

Connect the e adapter and computer with a USB cable, open file *M43toEF\_Expert\_Tools\_V1\_0\_0\_20160205.exe* (password:67240872), Click “search” button, it will show Model, current version and Serial ID

Choose “0.7×” below “Optic Reducer” and click “Write” button



Open file KiponM43toEF\_V2\_9\_0\_20170928.exe, it shows as follow



Click “Search” button,it will show Model, current version and Serial ID and then click “Update FW” to finish the update.